

Bill of quantities conference hall

	ITEM No.
	DESCRIPTION
BILL OF QUANTITIES FOR A COMFERENCE HALL
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SUBSTRUCTURES
Excavations and Earthworks 
Excavate oversite average 2500 mm deep to remove vegetable soil, load, wheel and deposit 100 meters away and later spread and level on site where directed.

Excavate to reduce levels starting from stripped level and column pits not exceeding 2.5M deep. 
Trim and prepare bottoms of excavations to receive blinding. 

Remove surplus excavated material and cart away.
Return fill and well ram selected excavated material around foundations
Fillings
Approved murram filling to make up levels, well rammed and consolidated in 150mm thick layers.

300mm thick approved hardcore filling spread, levelled, well rammed and consolidated in 150mm thick layers to receive concrete surface bed
Level and blind surface of hardcore with 50mm quarry dust to receive concrete surface bed.
Anti - termite treatment as "Premise 200 sc" distributed by High Chemicals essentials or other equal and approved applied to surface of blinded hardcore and surrounding areas strictly in accordance with manufacturer's instructions (subject to a TEN
YEAR GUARANTEE to the satisfaction of the Architect.)

Mass Concrete class 15/20 J 50mm Thick blinding: under foundations



DESCRIPTION

SUBSTRUCTURES CONTINUED
Vibrated reinforced concrete class 100/100mm in;
Strip foundation
300mm Thick ground floor slab

Sawn formwork to: 
Sides of strip foundations 

Edge of floor bed 75-150mm high 

Reinforcement
Fabric Mesh reinforcement 
Fabric mesh reinforcement to B.S. 4483 ref: A93 weighing 2.22 Kg per square meter in floor slab (measured net - no allowance for minimum 230mm laps) including tying wire and supports as required

Foundation walling
Rough dressed natural stones or other equal and approved bedded and jointed in cement sand mortar (1:4)
250 mm thick walls 

Hessian based bituminous felt or any other equal and approved dump proof course:-
 
Horizontal: 200mm wide.  

1000mm gauge polythene dump proof membrane with 300mm welted lap under concrete. 

Plinths 
150mm thick mortar cement and sand (1.4) rendered to plinths 

Prepare and apply three coats of bituminous: Ditto 
 

TOTAL FOR SUBSTRUCTURE CARRIED TO SUMMARY


DESCRIPTION
SUPERSTRUCTURE
WALLING
Masonry walls bedded and jointed in cement and sand 1:4 in: 

300mm thick wall reinforced with 32x2 mm hoop iron every alternative course

Provide 100mm pipe vents in beam above all doors with wire gauze and 25mmx400mm approximately in all windows upper middle compartment as permanent ventilation 

Ring beam
Concrete class 20/20 for tong beam

Reinforcement 
High yield reinforcements bars 
       Y16
       Y10
Binding wire
Formwork
Sawn formwork for lintel
  


DOORS
Double door with transom size 1500x2100mm high (D1 External door) 1.6mm thick middle rails complete with handles bracings to and all necessary accessories(ironmongery) including priming with one coat of red oxide primer before delivery to site and all weld grounds.

Timber door inclusive of architraves, quadrants, locks, hinges and door frames  


WINDOWS
Supply and fix steel casement windows consisting of standard Angline section frames and square rodes primed with one coat red oxide complete 



 
DESCRIPTION



10mby 2.5m high  (W1)
5m by 1.5m high(W2)
0.8by 0.8m high  (W3)
Inclusive of brushes
 
Glazing
5mm thick clear sheet glass and glazing to metal in metal patty in panes 0-10 – 0-50 square meters
Ditto obscure glass ditto 

Window board
Wrot cypress
125x25mm window board
20mm quadrant

Curtain rods
25mm diameter chrome rods
20mm diameter chrome net rod

Painting
Touch up manufactures priming coat prepare and apply two undercoats and one finishing coat gloss oil paint to:-
Glazed metal surface (measured Ove glass)

TOTAL COLLECTION FOR SUPERSTRUCTURES CARRIED TO SUMMARY

ROOF CONSTRUCTION
Slab roofing inclusive of all metal rods and painting









FINISHES
Internal wall finishes
40mm thick 1:4 cement sand render to wall
DESCRIPTION
30mm thick cement screed to wall  
Wall tiles
250 by 200mm wall tiles
Cement
Grote white
Painting
Prepare and apply three coat first quality 
plastic emulsion paint to:-
Internal walls

External wall finishes
40mm thick 1:4 cement sand render to ring beam

Painting
Prepare and apply three coat first quality plastic emulsion paint to;
Ring beam



TOTAL FOR WALL FINISHES CARRIED TO SUMMARY


FLOOR FINISHES
40mm thick 1:4 cement and sand render to floor 
5mm thick cement screed to floor 
Floor tiles
300mm square floor tiles
Cement tiles
Grote white

TOTAL FOR FLOOR FINISHES CARRIED TO SUMMARY











Electrical Installation Works

Allow a prime cost sum of Kenya shillings one hundred thousand for electrical works

Mechanical Works
Allow a prime cost sum of Kenya shillings one hundred and thirty thousand for mechanical works. 
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