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Name several operating systems that run LANs today
Cumulus Networks
The Cumulus Linux runs the LAN today. It is distributed by Linux and can use a variety of commodity hardware to operate (Internet source: Packet Pushers, 2017).
Big Switch Switch Light
The switch light is closely developed to integrate with whitebox hardware. It is an SDN-Centric NOS. It possess Open Flow-Like functions that enables it to operate on today’s switching silicon for data center. It is built on linux (Internet source: Packet Pushers, 2017). 
Open Network Linux
ONL is distributed by linux. It operates on “bare metal” switches i.e. commodity components with network forwarding devices. To install one has to use ONIE onto on-board flash memory (Internet source: Packet Pushers, 2017).
PicOS
PicOS can run bare metal switches from different manufactures. It is distributed bundled with its own whitebox switches or separately. It has both routing and switching support for the existing networks (Internet source: Packet Pushers, 2017). 
OcNOS
It is an enterprise and data center network. It has advanced capabilities that enables it to support Multiprotocol Label Switching (MPLS). IPFusion is OEMing the operating system to become more of vendor networks (Internet source: Packet Pushers, 2017).
Open switch
[bookmark: _GoBack]It is an open network source OS. Currently it is operated by Linux foundation. It uses the following platforms; Broadcom, VMware and Arista (Internet source: Packet Pushers, 2017). 
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