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Question 1
The maximum staircase riser should be 7 inches, and the riser height should be vertically measured between the adjacent treads of the leading edges per R1009.3
Question 2
The minimum fixture clearance for a water closet should be 60 inches when perpendicular measured from the sidewall and 56 inches perpendicular measured from the rear wall as per R604.3.1.
Question 3
The minimum corridor width should be 44 inches as per 1018.2
Question 4
The minimum footing width for a two-story conventionally framed home on soil that is 2000 PSF should be 15 inches per R403.1.1
Question 5
As per R802.7.1, the notch should be a maximum of a sixth of the 2×10 dimensional lumber floor joist and should not be longer than a third of the depth of the 2×10 dimensional lumber floor joist. Additionally, it should not be placed in the middle one-third of the span. Therefore, the maximum notch should be 2 inches to the bottom or top of the lumber floor joist. The hole should also not exceed 2 inches to the notch.
Question 6
As per table R602.3.1, the maximum height for a 2×6 wall stud spaced 16 inches should be 8 feet for exterior and load-bearing walls or 10 feet for interior walls and non-loading walls.
[bookmark: _GoBack]In cases of snow loads being equal or less than 25 pounds per square foot and the design wind speed equal to or not more than 130mph, studs supporting a roof load with less than 6 feet tributary length should have a maximum height of 18 feet when spaced 16 inches at the center or 20 feet when the spacing at the center is 12 inches.
