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OSHA Standard on Eye and Face Protection. Standard Number: 1910.133
Answers
1. ANSI stands for the America National Standards Institute.
2. These standards help ensure personal eye and face protection devises provide the necessary protection from the liquid plash exposures, non-ionizing radiations and physical impacts.
3. The years the ANSI Z87.1 standards were updated in the years 2010 and 2015.
The update purpose was to enhance product performance and attempts to come up with standards that are compatible with the international ones while minding the end users considering the workplace and regulatory obligations.
4. To ensure eye protection of safety the glasses as expected, the ANSI Z87. 1 certified the glasses to undergo the following tests;
· Basic and high-impact for the frames and the lenses of the glasses
· Exposure to non-ionizing radiation and chemicals
· Durability of flammables and corrosion
5. Summary of the video
The video is about the high mass impact tests as per ANSI requirement. The tests are done in the Colts Laboratory talked through by Daryl Neely. Glass samples are tested on the High mass impact test and the Dart penetration tests. The glasses are then rated with those resisting the impacts and penetration of the falling objects in the respective tests as “safety-rated eye wear”. On the other had those that didn’t resist are rated “non-safety rated eye wear.” Consumers are advised to take glasses that have passed the tests. According to the video, the ANSI. 235 allows them to request for tests before buying.
6. Product markings.
	Product marking
	What it means

	Z87+
	High-velocity impact

	D3
	Splash

	D5
	Fine dust

	W
	Welding

	U
	Ultraviolet light

	R
	Infrared light

	L
	Visible light filter

	Z87-2
	Prescription

	H
	Head size

	V
	Other( photochromic and s for special lens tint)



