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10 points each
	Air Quality Sampling Device
	Operating principle

	Example:               Denuder
	Pulls air through a hollow tube coated with a sorbent to measure gas and particulate phase pollutants together

	Bubbler
	The form of gaseous species that undergoes hydration to form an anion. More often used when fewer samples are required.

	Summa canister
	Collects air, in its gaseous state, in a pre-evacuated flask, to transport to an analytical laboratory.

	The continuous emission monitoring
system
	The immediate surrounding of air is taken from the monitor by sampling various chambers or holes. As such, the monitor would end up collecting or extracting a small amount of the air from the manifold to analyze by an automated technique.

	Passive sampling system
	A system that does not involve active air movement. Measures exposure levels in general communities. The system generally used for gases and vapors since particles are assumed not to diffuse






