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Design considerations

 Best way to distribute the internet connection to the boxes.
Switch and the routers connect with network cables and provide a wired connection point which links all computer devices into the SOHO network. Indirect access methods and internet connection is the best way to distribute internet. Use of Ethernet and wireless connection connects devices and the network connects with the internet. The use of a good mesh networking kit will save the business from the need to run a lot of Ethernet cabling. This will improve the performance of Wi-Fi since it will reduce devices number competing for wireless bandwidth
Wi-Fi access located throughout the premises
Wireless router provides wireless access points throughout the premises via the wireless router. The access points are mostly placed where most people in the office are using the network which reduces the costs of having multiple access points. This is done by selection of the right Wi-Fi access points. The Wi-Fi access point is added more antennas which leads to better reception and transmission. Besides an evaluation of Wi-Fi signal strength will offer the best strength throughout the office whenever one needs connection.  
 Determine how the SOHO network will be secured. 
Setting up credentials for wireless networks such username and passwords for wireless network. 
Setting up encryption mostly WPA-2 since it is the most secure.
Enabling MAC filtering for the network infrastructure to determine who can access the network.
[bookmark: _GoBack]Network Address Translation(NAT) is implemented by addition for more static addresses which reduces the risks of intrusions.
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