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Safety and health of all stakeholders of Stellar including customers is key to the organization. All employees are encouraged to observe the guidelines provided to ensure maximum safety in the workspace. However, significant hazards may occur in the workspace. To begin with, welding tanks may cause fire accidents since they are flammable. They ought to be treated with utmost care. The hoses and regulators, if removed in a careless way are likely to leak and cause fire hazards. Therefore, they should be properly stored.
 The tanks not in use should be properly stored and separated from the rest. In case of any fire hazards, fire extinguishers and protective clothing are provided for protection. Mechanical injuries may occur to individuals dealing with machines and mechanized equipment. Only trained personnel should be allowed to operate machinery. The operator should observe safety guidelines such as putting on seatbelts and observing the load capacity indicated for each machinery. The operator should not allow untrained personnel aboard to ride or operate the equipment or machinery. 
[bookmark: _GoBack]During concrete and masonry work, concrete buckets and masonry walls are likely to fall on construction workers. Furthermore, concrete dust generated by chipping or grinding of concrete work can be inhaled by workers. Workers are advised to put on protective gear such as dust masks to reduce health complications likely to arise from the inhalation of dust. No personnel will be allowed to work under concrete buckets. All masonry walls will be braced to avoid collapse. Employees working from a height can fall from ladders or roof edges. They are therefore advised to observe fall protection guidelines and safety plans to avoid injuries from falls. These include but are not limited to putting in place all elements of safety protection system. Lastly, personnel dealing in steelworks may be exposed to fall hazards. These are avoided by pre-planning of key elements and engaging fall protection systems.
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