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SITE SPECIFIC SAFETY PLAN 

Student Name

Institution Affiliation 

Submission Date

Continental Construction Company
453E. Horizon Building

Houston, TX 77202

Infix Installers & Finishers
This is a four storey building with 50 commercial offices and 6 restrooms on every floor. The task subcontracted for is to undertake interior build out which comprise of:

· Finish
· Drywall 

· Paint 

· Framing

· Tape 

· Finish 

During the course of work, it is expected that you will interact with a number of people within the building, namely

· Horizon Wiring & Electronics – will be fixing electrical fixtures within your framework.
· Milner Advent – will run air ducts beside heating and cooling fixtures

· Hemi Plumbers – will complete plumbing along the fixtures with the frame

· Millennium Levelers – will install floors

The Continental Construction Company safety orientation notes for the building are attached for your preview.

Site Specific Safety Plan
Read each section carefully and acknowledge by signing at the end of orientation
SDS Sheets:

1. The SDS sheet should always be presented to Superintendent prior to starting work and also before ferrying any chemical to the construction site.

2. All chemicals to be used on the site must be labeled clearly.

3. Empty chemical containers must be disposed safely in accordance with SDS sheets.

Orientation and safety meetings

1. Every worker expected to work on the site must attend orientation.

2. Site sticker is issued to every employee that has attended the orientation to confirm he understand the safety measures and necessities of the project

3. Any worker using false pretence as a result of policy violation may be banned permanently from ANY CONTINENTAL PROJECTS. Provision of Personal Identification and passport photo is mandatory.
4. Foremen are expected to be present at weekly safety meetings

Accidents

1. All accidents within the sites and any likely misses should be reported to Continental Construction Supervisor
2. Every subcontractor is expected to submit an incident assessment report with corrective measures for near misses or accidents with 2 working days after the event. 

Emergency Action Plan

1. Continental has placed emergency action plan on the site

Fall Protection

2. Protection gear should be used for fall protection especially those working in elevated places.

3. Handrails and cables should be protected and if removed for some work by subcontractor, they must be reinstalled thereafter as per OSHA requirements

Excavations

1. Excavations with depth of six feet and above need to be barricaded, especially where view seem to be obstructed

2. Excavations with 5 feet depth or above need to be benched, shored or sloped in accordance with OSHA guidelines
3. Excavations work will only be awarded to competent people referred by subcontractors
Site Specific

1. No weapons, fighting, alcohol or drugs are allowed on a construction site

2.  No radios or loud music is allowed
3. Drug test is a must to all workers in the site

4. Subcontractor is liable for any misbehavior of his team

5. Subcontractor must avail drinking water for his team

6. Smoking is not allowed on the site

Fire Prevention

1. Metal gas cans are the ones to be allowed on the site. NO PLASTIC CANS!!

2. Suitable fire extinguishers must be available in working location. 

3. Gas cylinders need to be well secured, stored in upright position

Electrical

1. Extensions cords to be used in the building must be three-wire type
2. Electrical equipment must encompass GFCI outlets 

3. Lockout need to undertaken at the exact source of power and linked to the device.

4. Light fixtures should be secured ones they are installed

5. Circuit breakers boxes need to be marked with signage reading “Danger Electrical Hazard”

Barricades
1. Red Danger tape should not be crossed

2. Warning line must be used in places that need caution

3. All signs used on the site must be observed

Motorized construction vehicles and cranes 

1. Will be operated by qualified operators

2. Seat belts must be worn

3. Cranes must have inspection certificate

Enforcement

1. Each subcontractor is independent and must manage his workers

2. The construction site has zero tolerance to any deviant behavior
3. Willful unsafe acts may lead to termination of subcontractor contract.
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