To test the water permeability of the assembly, a standardized CSA A440 water penetration test was conducted. This test has two components: A static test and a cyclic test, in order to evaluate the window’s performance in different situations. The static test sprays a constant stream of water at a set pressure for a given period of time, whereas the cyclic test is performed in short intervals. 

5.1 Instrumentation

To perform this experiment, the following is required:
1. Wall/Window assembly
2. Polyethylene sheet and tape
3. Manometer
4. Spray Rack
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