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Wireless Sensor Networks
Introduction
	The current technology has brought about radical transformation of every aspect of life. Information technology, medical, and engineering fields have quite benefited from technology evolution. Introduction of sensors is the fundamental of automation that today most of electrical appliances operate from. Precisely, sensors are devices that detects and responds to physical conditions or environments such as heat light and pressure and convert them to electrical signals under some control that enhances further processing. The ability of sensors to transmit signals give rise to both wireless and wired networks used in various fields such as artificial intelligence, surveillance and Machine control. Basically, wireless sensor networks (WSN) are networks formed through interconnection of devices that share or communicate information sourced from monitored fields that has wireless links. It normally consists of various components such as nodes and the base stations that work together to create the desired output. Since WSN are among the most recent technology usable in various automation, it is important to explore and analyze how they work by addressing some of its components such as network technology, routing, hardware and software platforms, applications and security among others. 
Wireless sensor network technology
As seen earlier, a wireless sensor network is an interconnection of various devices such as sensors, nodes, processors, detectors and low power antennae’s. Among this the sensor node is the most important element since it enhances communication with other nodes. Since many automations are aimed at creating efficiency, there are characteristics that they must exhibit for them to be considered efficient (Kamal, 2005). In this case, the characteristics of a good WSN is defined by scalability, power efficiency, responsiveness mobility and reliability. Scalability refers to the ability of a network to grow without causing overhead. Power efficiency refers to the networks ability to handle changeable data paths and mobile nodes. Responsiveness entails the ability of a network to timely adapt to changes in the topology (Zheng, 2008). Reliability is the ability of a network to carry out desired operations without bias in that it should be able to transmit and maintain data in a continuous network structure. Lastly, mobility entails the ability of a network to handle changeable data paths and mobile nodes.
 Network architecture is the organization or framework of a network. Most of the WSN networks follow the OSI model that consist of five layers including, application, transport, network, data and physical layer. It also consists of three cross layers that is, carry task management plane, mobility management plane and power management plane. Each of this layers have a specific function that contributes to the network framework operation. The physical layer is responsible for generation and selection of frequency, modulation signal detection and data encryption. The application layer is responsible for traffic management and software support that enhances conversion of data into positive information. The transport layer enhances reliability and delivery of congestion avoidance (Moradi, 2012). The network layer is responsible for rooting while the data link is responsible for data control, multiplexing as well as enhancing reliability of point to point transmission. The hardware and software platforms are used to as host in the WSN. Basically, the most usable hardware are controllers, external memory and sensor nodes.  On the other hand, the software platforms are operating systems that support the node hardware. Unlike general purpose systems that uses windows and Linux, the WSN uses tiny operating system known as nesC and uses C language to support driven based programs. The main application of WSN networks are industrial processing, machine control, and artificial intelligence.
                                      Mobile wireless sensor networks
Mobile wireless sensor networks are modification of sensor nodes within a network. It has a mobile sink designated with various nodes that show different commands. The nodes have different characteristics. For example, those designated with orange colour show nodes that are directly reachable by sink. The colorless ones show nodes reachable through multihop communication. Those in purple designation shows nodes that assist the mobile sink to collect data.  The network structure of the mobile WSN consist of three units that is power unit, processing unit, transmission unit and sensing unit. It has other components such as the memory, transreciever, the mobilizer, the sensor the antennae and the location finding system. All coordinate to give the system update. Nodes are devices that operate within a block chain network, their main roles are to support the network, process transactions and secure data through hashing (Zheng, 2008). The challenges that affect the mobile wireless sensor networks are Node deployment, link heterogeneity, data delivery model, energy consideration, scalability, coverage, network dynamics and fault Tolerance. Node deployment challenges the mobile WSN by affecting the routing performance based on the type of node deployment used. 
Node heterogeneity leads to technical problems caused by overhead and some data routing. Energy consideration factor is a challenge in that routing requires efficient energy which at times can be in efficient (Moradi, 2012). Fault tolerance is subject to environment limitation in terms of range and accuracy. Mobility models are used in ad hoc wireless networks. In mobile WSN they are used to assess whether a given protocol is usable or not. Generally, there exist three types of usable mobility nodes. They include, mobility of sensor nodes, mobility of sink nodes and mobility of monitored events. Their difference lies between how they occur in a mobile. For example, the mobility of sensor node occurs when some parts of the sensor nodes are mobile. On the other hand, the mobility of sink nodes occurs when a node is able to automatically move in the next region to source data from a sensor network.  The mobility of monitored events happens when the mobile wireless sensor network is used to for tracking purposes which works through data models driven by the system. Therefore, it can be said that the mobile wireless sensor networks employ an integration of various components used in the WSN architecture. 
Routing in Sensor Networks
Routing in sensor networks entails moving packet data from one host to another. As much as routing is important in WSN, it is subject to some challenges that affect the design of routing protocols among other networking processes.  In this case, the routing challenges are tolerance and scalability, data transfer, networking design, energy consumption, and node deployment. Tolerance and scalability is an effect that occurs when the nodes of the sensors fail due to loss of power or malfunction of other external components. If a sensor or a node is scalable it should be able to respond to the events irrespective of power failure or malfunction. However, most nodes and sensors are not scalable and this creates a challenge   in case of other component malfunction or power loss.  Node deployment has an effect on the functioning of the network protocol. For example, where nodes are not uniform, optimal clustering is required to enable efficiency in network operation (Zheng, 2008). In terms of energy consumption, power becomes a challenge when the lifetime of a battery supporting the sensor is not certain. The type of networking design used also creates some challenges in that some considerations must be made while designing the network topology or the routing to be used. It happens that when the network design is improperly made, it may lead to message traffics that may cause instability in the entire system. In networking, data transfer becomes a challenge when the routing method is not quite effective. It means that to have effective data transfer, data receiving and transferring must align with the routing system employed. 
Routing protocols are rules set by routers in the determination of the most appropriate paths to deliver data in the required destination. Generally, there are various protocols used in WSN. Among them are routing information protocols, interior gateway protocols, open shortest path first, exterior gate protocols and border gateway protocols among others. However, all are categorized into three main protocols which include, Distance vector protocols, interior gateway protocols and classless protocols (Kamal, 2005). The distance vector protocols are characterized by sending the whole routing tables through the analyses, sending periodical updates of less than one minute as well as broadcasting updates. However, it is prone to routing loops. The major category of distance routing protocols is routing information protocols and interior gateway protocols.  On the other hand, the link state protocol is characterized by providing link state information and use of triggered and multi casts updates. It has no effects of routing loops and are commonly used in open shortest path first and intermediate system to intermediate system routing designs. 
The interior gateway protocols are distance gateway protocols that are produced by Cisco, they function effectively in larger networks. In their functions, they use metrics such as delay, reliability, and bandwidth. The classful and classless protocols differ in terms of update sending where there is no mask information send during the routing updates while in classless there is information send during the routing updates. The ability of the classless protocol to send mask information during routing made it to outdate the classful protocol usage in wireless sensor networks. A network structure is an organization based network that is considered as less hierarchal, flexible and more decentralized. In this case, the network structure is divided in three protocols that is flat routing, hierarchal and location based routing. In flat networks, the nodes play similar roles as well as collaborating in the sensing task. The routing based protocols operates in a multihop sensor network where it performs two major functions that is forwarding data packets through the routes and finding the routes that leads to the sink nodes (Zheng, 2008). The hierarchal routing entails arrangement of routers based on hierarchies. It functions that each router saves some information about the other routers.
 Increase in the number of routers increases the network size and the network table graphs. When the network grows to a certain size it creates a network traffic that the routers cannot handle. It is because of this predicament that hierarchal routing is introduced to overcome the barrier of network traffic. In this case, algorithms are used to find routes between the nodes while the routers are classified in terms of regions. The location based routing protocols, operate based on the location information of the nodes that is. communication is made with regard to the node location. In WSN it is also known as geographic routing protocol. In its data transmission, packet forwarding and route discovery is done with regard to location information. In wireless network transmission, it is quite used since it has advantages such as controlled overhead, save on energy consumption, less memory required and it is also scalable (Moradi, 2012). Besides, it has also different types that gives alternatives of different features. The most common alternatives are minimum energy, communication network, greedy perimeter stateless routing protocol, and small minimum energy consumption network. Each has distinct features that are considered based on the type of routing or data transmission selected. In WSN, network protocols define conventions and rules used to communicate by the system devices. It usually uses the OSI model and is divided into different categories such as internet protocols, wireless network protocols, and network routing protocols. In this case, the protocol specification defines the protocol operation. It means that the feature that defines the protocol determines its operation and perhaps the model of the protocol. 
 Generally, it consists of three parts that is, definition of protocol control information, definition of procedures for receiving and transmitting PDUs as well as definition of services that are provided by the protocol layers. In WSN, the protocol defines the operation, for example, it determines how the protocol data unit is processed at transmit and receive nodes. In this case, the protocol operations create specific valid values for the PDU header and the actions taken at the reception of PCI value. Some of the operations implemented in protocols are segmentation, flow control error management, and connection management. Notably, in WSN these operations function with respect to the three model layer that consist of link transport and network layer. As seen earlier this protocols define operations (Zheng, 2008). For example, in the wireless network protocol, the protocols are designed to support roaming mobile devices and other issues such as network security and variable data rates. Negotiation based routing are type of protocols that uses negotiations and data of high level to eradicate data redundancy transmission. It means that this protocols harmonizes data between hosts that tend to appear similar in separate entities. 
Alternatively, in wireless sensor transmission, spin nodes can also be used to make communication decision. However, application of specific knowledge of the data and resources must be included. The reason why knowledge and resources are emphasized in this notion is to enable sensors to evenly distribute data when provided with a limited data supply (Zheng, 2008). Notably, the process is conveniently usable for both broadcast and point to point network. The query based routing is a typical protocol process whose design considers both distance and energy when routing data packs across networks. It is an advantageous method in that it helps balance loads in different sensors. As such, the sensor is protected from running out of power while the routes to data destination are kept relatively short. In its operation in a wireless network, it functions by sending queries to find specified events in the WSN. During the transmission, two strategies are used and entail energy balance and energy savers. Both strategies aim at balancing and reducing energy consumption that help prevent network partition. 
In wireless sensor networks, data can be transmitted using many paths created in a network. Multi hop paths have been extensively used in data routing however, recent studies suggest that they are limited in capacity and the dynamic of the wireless links have been reported to be inefficient in data rate transmission (Moradi, 2012). Discovery of multipath routing in wireless transmission helps eliminate this problem by improving the performance of wireless sensor and the ad hoc network. The quality of service routing is a type of network routing that depends on preferential service delivery applied to reduce packet loss, control latency and ensure sufficient bandwidth.  In WSN coherent based routing is also usable in data transmission. It functions by forwarding data to aggregators after the preliminary processes such as duplicate suppression and time stamping. In most wireless networks it is used due to its ability to save on energy. 
Security
Like any other transmission, wireless security is prone to security threats that are inherent to the sensor node system and the external transmission. Studies highlight that wireless networks are prone to security threats like unguided transmission medium. Generally, attacks in WSN are viewed in two fundamental perspectives that is, threats against security mechanism and threats against basic mechanisms. The major attacks are denial of service, attack on information in transit, Hello flood attack, wormhole attack, and Black hole attack (Dargie, 2010). In routing heat and run attacks are very common and attack specific network or router. The denial of service request uses stray requests that floods the network with unnecessary information thus distorting the required one. Attacks on transport layer in the framework protocol of WSN are denial of service Sybil and blackhole attack. Privacy attacks are Trojans, sniffer spyware, and key logger. Trojan attacks the network and hardware platform of a network. Sniffer attacks the packet data across the network during troubleshooting. The spyware attacks the surfing information such as network configuration. 
To evade this security threats, it is recommended to use methods such as firewalls, passive capturing, data encryption, authentication, and content filtering among others (Zheng, 2008).  Firewalls prevent unidentified success in both wired and wireless transmission. Authentication secures data in a network by use of password. Data encryption entails transforming data into another code such that it is unidentified when passing through a network. Content filtering entails sieving network information that can be accessed to create room for attacks. Use of intrusion detection is also an effective method that entails installation of a software in wireless networks to provide software intelligence to all sorts of network threats.

Conclusion
To sum up, it is quite clear that wireless sensor network is a wide field that entail interconnection of devices to enable wireless data transmission. Despite being associated with numerous challenges, its application is still wide and prominent especially in artificial intelligence a machine appliances. It is also found that networking in WSN is a major component that addresses the concept of data transmission and protocols observed during the transmission. Short energy saving and efficient data paths such as multipath based routing are quite effective in data transmission since they help overcome overhead and data redundancy. Lastly, security threats such as denial of service Trojan and hello flood attack has been found to be common in networking however, by using firewalls data encryption, and authentication measures the threats can be eliminated to enhance smooth flow of data packets. 
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