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1. The solar cell is responsive to a particular wavelength or color of visible light. The yellow color is the most robust absorber of view because it produces the most significant current of 5.5mA while red color is the second absorber of light. It generates a flow of 5.0Ma. The blue color is the third one it makes 4.3mA and green color is the least absorber of view because it produces the smallest current of 3.8Ma.
2. The solutions of the beaker are 
	



Standard / known solutions
	
Beaker 
	
Concentration.

	
	
1  
	0.2

	
	
2 
	0.4

	
	
3 
	0.6

	
	
4
	0.8

	
	
5 
	1.0












3. 

	

	
Beaker 
	
Current ratio 
	
Absorbance.

	

Standard / known solutions
	
	
	

	
	
1
	0.8333
	0.0792

	
	
2
	0.6667
	0.1761

	
	
3
	0.5000
	0.3010

	
	
4
	0.3333
	0.4772

	
	5
	0.1667
	0.7781

	Unknown solution 
	6
	0.250
	0.6021



4. Graph 
5. 0.8240 (ppm)
6. I prefer yellow color. It is the best color that absorber more light compared to the other color.

