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Kang, (2018) suggest that over the last few years, we have experienced high incidences of falls at construction sites. It's the responsibility of the employers to prevent falls on a construction site. Fall protection falls under two categories; active and passive fall protection. All active fall protection for the construction sites fall under four categories; fall arrest, fall positioning, fall suspension, and fall retrieval. On the other hand, passive fall protection is a system that is nondynamic, stationary, and does not adapt or move or change when in use or out of service. Therefore, there is a need for proper fall protection in all construction sites by maintaining a harmless working environment through appropriate protection education, appropriate personal defense, and adequate training.
According to Kang, (2018), failure to implement these fall protections would result in the following hazards. Some workplaces have wet floors; therefore, walking on wet floors inside or icy floors outside the construction site can cause the workers to slip and eventually break their bones. Other workplaces don’t have personal protective clothes causing the workers to fall from great heights of above four feet due to climbing high cliffs without wearing an appropriate harness or proper fall protection, causing breakage of bones and even death to the workers. Working in a workplace without fire extinguishers can result in body burns in case of a fire outbreak. Additionally, some workers don't know how to use the fire extinguishers and may eventually suffer burns in an episode of fire. Workers working in a workplace without lifting or moving machines carry heavy loads, finally breaking their bones. Additionally, some workplaces have forklifts and stationary objects, which end up crushing the workers. Some workplaces don't have proper air ventilations exposing the workers to poisoning through inhaling hazardous chemicals, mainly while mixing harmful them. Additionally, lack of personal protective clothing like a mask in a workplace exposes workers to poising while mixing toxic chemicals.
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