Flow chart for a jumping "dead" car battery
Switch off the
 ignition and open
 the hoode of the two cars

Park active vehicle
 near to the one 
with dead battery

Loacte the car
 batteries and
Get the jumper cables



		
[bookmark: _GoBack]Does the ingine start?

If it fail to start again next,
 it means the battery does not 
store charge and should be replaced.  

No: Check if the jumper
 cables are connected properly. 
If it does not work still,
 consider replacing the battery

YES: drive the car
 for about 20 minutes
 to let it charge the dead battery
Try to start the 
ingine of the car
 with dead battery

Attach the other
 red clip to the
 positive terminal 
of dead battery

Start the ingine 
of the active vehicle
 and let it run 
for few minutes

Attach the black clips 
on negative terminals
 one on the ative battery
 and the other one at 
the dead battery

Attach one red
 clip of the jumper
 cable to the
 positive terminal of active battery


