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	GENERAL
All dimensions are in mm unless otherwise specified. Drawing are not to scale only figured dimensions to be used.
The contractor must check and verify all dimensions before commencement of any work. CONSTRUCTION
All slab at floor bed to be poured over 1000 gauge polythene sheet on 50mm thick marrams blinding on hardcore. All soils under slab around and under foundation to be poisoned for termite control.
CIVIL

All soil on cut embankments to be stabilized. The slope not to exceed the natural angle of repose STUCTURAL
All black cotton soil to be removed from all buildings and paved surfaces.
For all R.C work refer to structural Engineers details
Depth of foundation to be determined on site to
S.E approval
All walls less than 150 mm thick to be reinforced with hoop iron at every alternate course.
All adjacent R.C work and masonry walls to be tied with strip iron every alternate cost.
MECHANICAL

All plumbing and drainage to comply with relevant local authority.
SVP to be provided at the head of the drainage system.
Drains passing beneath buildings and driveways to be encased by 150mm concrete surrounding.
The storm drain pipes to comply with BS 556 specifications.
All underground foul and waste drain pipes shall be UPVC to comply with BS 5255.
All inspection chambers covers and framing shall be cast iron.
Minimum slope in the drains pipe to be 1 in 100. No chases will b allowed for pipes.
All testing of pipes must be completed before plastering.
All mechanical works must coordinated with electrical and any conflict must be clarified before work begins.
PV denotes permanent ventilation.
ELECTRICALS

All conduits must be laid before plastering.
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