
[bookmark: _GoBack]A standardized CSA A440 water penetration test was carried out while testing the assembly’s water permeability strength. A cyclist test and a static test are two key components which play a vital role in this test with the aim of evaluating the performance of the window in different platforms. A constant stream of water is sprayed by the use of the static test spray at a given pressure for a certain period of time.  For the cyclic test, the performance barely takes some short time intervals. 
 
Apparatus
The following are some of the primary instruments required to conduct this experiment. 
i. Spray Rack
ii. Polyethylene sheet and tape
iii. Manometer
iv. Wall/Window assembly



