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Answer Question Lab 1-26
DEFINITIONS
1. Inductance
Refers to the tendency of a given electrical transmitter to resist change in the electromagnetic current transmitted through it (Wu et al., 2018).
2. Henry
Is the mutual-inductance or self-inductance unit named after a scientist known as Henry?
3.  Inductor
An inductor is a double terminal passive electrical component.
4. Choke
Refers to an inductor whose main role is blocking higher frequency while transmitting a direct current as well as lower lying frequencies of the alternating current in a given circuit.
5. Domains
A region characterized with magnetization in a similar and unique direction, for example, ferrimagnetic domains (Wu et al., 2018).
6. Time constant
Time factor representing the responding speed of a given system as per a specified parameter.
QUESTIONS
1. What letter symbol is used to represent inductance?
Inductance is represented by the letter L.
2. What is the unit of inductance?
The SI unit for inductance is Henry.
3. What letter symbol represents the unit of inductance?
Henry, the SI unit of inductance, is represented by the letter H.
4. Draw the schematic symbol for an air-core inductor.
[image: ]
5. Draw the schematic symbol for an iron-core inductor. [image: ](Wu et al., 2018)
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