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Galvanic Oxidation
[bookmark: _GoBack]Copper and aluminum are the materials discussed in the case study. With a reduction potential of -1.67, aluminum is the anion while copper is the cation at a potential of +0.34. This problem could have been avoided by using copper in the wiring. Since full-rewiring of all houses is not practical, special Cu/Al wires can be spliced to the aluminum wires to make contact with the copper panels. Moisture was part of the electrolytes in the reaction alongside air. 




