HOMEWORK 1
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1. Draw a lightbulb showing clearly cach part. Which parts are conductors and which
ave insulators? Include the path taken by charges and the direction.
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2. Which of the following circuits will light up the lightbulb?
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3. Sort the following circuits in

(a)

“series” or “parallel”
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4. Alightbulb of resistance 30 is connected to a 1.5V battery.
(a) Draw a diagram of the circuit.
(b) Use Ohm’s law to find the current (remember to include units)

(c) Now assume that the cireuit above has two lighbulbs in series, each with resistance
150, You will learn in future labs that this makes the current flowing through
the cirrcuit exactly the same as what you found in part b).

Using Ohm’s law for each lightbulb find the potential drop at each lightbulb.
What do you notice about the sum of potential drops? [Hint: If you know the
current flowing through and resistance of an individual component you can use
Ohm’s law for that component, i.e. Viomponent = Leomponent X Reomponent
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