Option 2 
[bookmark: _GoBack]The connecting wire must have a current of 3 A. This is according to kirchoff current law that state that current entering is equal to current leaving a wire. 
