Question 3
a) Earth Leakage Circuit Breaker
b) Multimeters
c) Megger insulation tester
d) Clamp meter
Question 6
a) It will produce an out of range reading which could be incorrectly presumed to be a correct reading.
b) Reversed polarity – having positive and negative around the wrong way.
c) Incorrect connection to the circuit such as connecting an ammeter in parallel
d) Use of a Multimeter with a broken test lead or an open circuit fuse.
Question 5
a) Checking the power consumed by an installation
b) Checking for overloaded cables in an existing installation
c) Checking a switchboard for loose terminations
Question 4
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