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Learning Outcome from the Article by Aage Bjørn Andersen.
The article highlights various issues on the procedure and various practices, which has been adapted to ensure proper disposal of obsolete ships. His great emphasis is on occupational safety and health issues, and various aspects within the environment are influenced during the ship breaking process.
Andersen mentions that, although the entire process of ship demolition is a dangerous and dirty occupation by all standards, breaking them in the beachheads remains unsafe. The price of the scrap metals and the existence of the ready market for all the recycled goods and products affect the feasibility of shipbreaking significantly.  The ILO's meeting in the year 2000 on the social and labour Impact on Globalization recommended that, first, the ILO have always to draw the best practices to be adapted to achieve a comprehensive practice on safe and healthy occupation in shipbreaking. Secondly, the government must be encouraged to ensure ships have an inventory of dangerous materials within their reach and have to be updated so long as the vessel is in use. All this will be able to ensure the safety and health of workers is assured and the entire environment. 
Policies on ship disposal
The European Union recently undertook economic and technological feasibility of scrapped vessels in Europe. All was done following several accusations of them breaching the Transboundary Movement of Dangerous materials and how they are disposed of. On the other hand, the US has prohibited the export of its vessels to the breaking majors. The above initiatives indicated that the entire world is reluctant to accept the present procedures for ship breaking. This affects job creation for those well-established countries in the vessel breaking areas.
Principle of the breaking process
The process of shipbreaking involves various chains of operation done in different places. Offshore, this involves emptying of tanks and valuables found in the ship. The inter-tidal zone is the second phase of ship breaking, which involves the entire vessel beached within its power and breaking initiated. The vessel is further cut into small manageable sizes at the beach as sorting is done for transport. The last step is done at the shore; already cut materials are supplied as second-hand equipment to the market, and recycling and manufacturing. 
Principles on the current Practices.
In most cases, the majority of the vessels heading to retirement are offered to be sold on the available scrapping markets. This involves selling it to the highest bidder.  Because of the available workforce and ready market for second-hand materials, the ship breaking and scrapping procedure has been based on the principle of maximum separation, which mirrors the reverse process of shipbuilding.
Collective Bargaining
Within the shipbreaking process, the employment rights tend not to exist, and thus the absence of the collective bargaining. The living conditions within the ship breaking process tend to mirror the full absence of norms and standards to be considered.

International Shipping-Expectations and resource Management
[bookmark: _GoBack]As it remains unacceptable to try exploiting workers by giving low pay, working in unsafe environment or by using under aged children as workers, likewise, it is unacceptable to dispose harmful wastes and substances to the environment and thus causing harm to the society and the entire environment.
Perceived Roles of Various Organizations.
IMO –Coordinates various issues, which are associated with ship recycling. This body also monitors issues resulting from shipbuilding, design, building and its operation that can influence recycling.
International Labour Organization (ILO) – Establishes operation standards in shore-based industries, all of which are involved in the entire process of ship recycling,
The Basel Convention on Transboundary Movements of Hazardous Wastes and their Disposal –It recognized the convention’s limited application to the recycled majority of ships with the aim of concentrating on identifying safe ways and methods of disposing of hazardous wastes.
The 1972 London Convention – Aimed at monitoring ship disposal at sea and was meant to encourage recycling as a preferable method. 
The industry – Develop an excellent code of good practice. 
Environmental groups – Monitors as well as reports on various issues during ship breaking and recycling. 
Nations –They develop, adopt and at the same time, they enforce appropriate and relevant international standards set on ship recycling or breaking.
International Transport Workers’ Federation/International Metal Workers Federation
The IMF remains to have been actively involved in all aspects of health and safety, and has always undertaken various measures during the entire process of ship breaking. The IMF department of shipbuilding work Group has been in collaboration with various trade unions rights within the shipbreaking sector.
In summation, the article clearly indicated that the practice of the IRs in the shipbreaking process is aimed at reducing the effect of the hazardous substance produced during the breaking process and protecting the health and safety of the workers. This is further done to protect the environment from the improper handling of the substances and items produced during the ship breaking process.


LINK: https://www.ilo.org/wcmsp5/groups/public/@ed_protect/@protrav/@safework/documents/publication/wcms_110357.pdf 
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