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[bookmark: _GoBack]The clay is classified as either medium or stiff in relation to it’s plastic consistency. The most common measure that is used to give the difference between medium and stiff clay is the oedometer test data. The first difference is that the thumb will infiltrate about 6 mm when the moderate effort is applied and is molded with strong finger pressure. On the other hand, the stiff clay intents effortlessly and infiltrates 12 mm when great effort is applied. Moreover, the undrained shear of medium clay ranges between 500-1000 lb/ft2 while stiff clay ranges between 1000-2000 lb/ft2.  
