Question 1
What do solid vertical lines in the margins within the body of the 2017 code mean? 
Group of answer choices

There was a technical change from the 2012 edition

Text has been relocated

Something was deleted from the previous code

There was a change in the base code
 
Question 2
What year did the State of Florida begin to mandate statewide building codes?
Group of answer choices

1990s

2000s

1970s

1980s
 

Question 3
What do dotted vertical lines in the margins within the body of the 2017 code mean? 
Group of answer choices

There was a technical change from the 2012 edition

Something was deleted from the previous code

There was a change in the base code

Text has been relocated
 

Question 4
Which of the following are exempt from permit: (choose all that apply).

Group of answer choices

Self-contained refrigeration system containing 9 pounds of refrigerant and actuated by a motor of .75 horsepower.

Emergency repairs

Portable heating appliance

Minor repair that does not affect something covered in the code

Replacement of any part of mechanical system that does not alter its approval

Chilled water piping within any heating or cooling equipment regulated by this code

Replacement of any part of mechanical system that alters its approval
 

Question 5
There is no section for earthquakes in the Florida Building code.
Group of answer choices

True

False
 
Question 6
The Florida Building Code DOES NOT cover: (click all that apply)
Group of answer choices

Construction of a new bank

Alteration of an office building

Temporary Set for movies

Federal Buildings

Repair of a four story condominium

Chickees

Enlargement of a fire station

Railroad Facilities
 
Flag this Question
Question 71 pts
If the code dictates different specific material or methods of construction:
Group of answer choices

The general requirement shall be applicable

The stricter requirement shall be applicable

The less strict requirement shall be applicable

The specific requirement shall be applicable
 
Flag this Question
Question 81 pts
Match the following:
Group of answer choices
Photovoltaic Module 

Photovoltaic Panel 

Photoluminescent 

Photovoltaic Panel System 

Photovoltaic Shingles 

 

Question 9
A shaped material, made principally from polypropylene homopolymer, or copolymer, which in some cases contains fillers or reinforcements, that is used to clad exterior walls of buildings.
Group of answer choices

Particleboard

Polypropylene Siding

Oriented Strand Board

Plywood
 
Question 10
Match the following:
Group of answer choices
Carbonate aggregate 

Cellular 

Lightweight aggregate 

Perlite 

Sand-lightweight 

Siliceous aggregate 

Vermiculite 

 
Question 11
If a structure is purposed for use not covered in the code: 
Group of answer choices

the structure shall be classified in a group that has the highest restrictions. 

the structure shall be classified in a group that best resembles the fire and hazard risk associated with the use.

the building must meet one of the categories of use or it cannot be constructed.

the structure shall be classified in a group that is chosen by consensus of the review board. 
 

Question 12
An arena with attached Business offices and a restaurant open to the public should be considered what occupancy group?  
Group of answer choices

A-2 and A-4

Group B only

Group B and A-3

Group B and A-2, A-3 and A-4

A-2, A-4 And Group B

A-3, A-4, A-5
 

Question 13
Air craft manufacturing facilities with office space should be classified in what group occupancy
Group of answer choices

A-3, F-1, F-2 and Group B

Group F-1 and Group B

Group F-2 and Group B

Group A-3

Group F-1
 

Question 14
What is the sq ft space requirement per person for a building in a mall with 30,000 sq ft of leasable space?
Group of answer choices

28

31

27

27.1
 

Question 15
What is the maximum occupancy for a building with 10,000 sq ft of leasable space?
Group of answer choices

400

300

390

389
 

Question 16
A building with Group I-2 Occupancy construction Type V A is allowed _______ sq ft of area per story.
Group of answer choices

9,500

14,000

12,000

15,500
 
Question 17
Where a building is equipped throughout with an approved automatic sprinkler system in accordance with Section 903.3.1.1, the value  for maximum building height is increased by _______ and the maximum number of stories is increased by one.
Group of answer choices

15 feet, two

25 feet , one

60 feet , two

20 feet , one
 
Flag this Question
Question 18
Your client is looking to build a structure. During the design phase they tell you they are not sure of the actual final parameters but the building will be a storage facility on the ground floor for different types of hazardous materials , areas on the first or a second floor for office space, and possibly a storage facility for other chemicals no hazardous. The owner is not sure if they want to go high rise or not but the minimum floor area for each level will be some where between  25,000 sq ft and 120,000 sq ft. The owner wants to know what are the code factors that might dictate the final building. Include references to the Florida building code. Think about what the owner will care about. Explain the consequences of each decision. Use examples from the Code to make your point. What types of construction are required based on the choices?
