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How to Specify Carpet
	The modification ratio compares the inner (y) and the outer (x) circles. When the ratio is low, it means the fiber contains a large surface area and fewer chances of trapping soil and other dirt. Notably, modification ratio affects carpet fibers' performance because whereby if the fiber is round, the ratio is low, meaning it performs better as chances for foreign materials like dirt are limited.
	It is a good idea to specify a solid carpet for heavy foot traffic areas such as the sitting room. They are durable as they hold their shape for long despite the traffic. The solid carpets are also less stained and moisture free, implying they rarely get dirty. As a result, the need to wash many times is reduced, making them retain the shapes longer.
	The minimum carpet density value for commercial applications is 5000 ounces per cubic yard (interiorandsources, 2020). The level recommended in these areas is more because a lot of foot traffic is expected. For example, the people visiting a mall are more than households, requiring the 5000 density level to ensure durability and reliability.
	Embodied carbon refers to the carbon mark in a material. It determines the greenhouse gases produced in the supply chain either at the factory or usage level. Cradle to the Grave is the reliable method to assess embodied carbon as materials from the ground level to the final stage are determined. With the increased environmental concern, the market and the governments emphasize the need to ensure the embodied carbon released is minimal.
	Green chemistry refers to chemical products and procedures designs implemented to lower or control harmful products' production. The model applies in the life stages of a chemical good from the designing stage to the disposal. The green industry is evident in the carpet industry, where principles like waste prevention and safe reaction conditions are ensured.
	The circular economy is a systematic model aiming at preventing wastes, so the resources available are used longer. Carpet specification entails aesthetics and appearance where a circular economy is applied. Normally, the more specifications are introduced, the more the market develops, making it possible to recycle and reuse the materials, thus meeting the circular economy's goals. 
	Carpet designers should prefer green products referring to those minimizing the effects on the environment. It would make them gain competitive benefits as the buyers prefer products with no adverse effects on the environment. Using green products also makes the companies socially responsible, thus reducing the costs of production. For instance, the products would be recycled or reused, thus saving money that would be used to purchase new materials. Additionally, it improves safety and health, an essential factor to consider while producing goods for buyers. 
	The coatings that are at times added to fibers for waterproofing and stain resistance are problematic. They lower the materials' strength and be re-gelling coated every five years, making it expensive. Moreover, they produce airborne fibers that are unhealthy to the users, especially those with asthma. The coatings also need gaps that make the fibers ineffective if the materials get wet during the installation process. 
	The institution providing generic standards for carpet installation methods is Carpet and Rug Institute (interiorandsources, 2020). The organizations make and implement laws on both commercial and residential carpets standards.
	Proper maintenance is essential to the durability of a carpet installation. The activities prevent soil accumulation that would destroy the carpet fibers. With that, its life is prolonged, and the costs of restoration are eliminated. The guidelines to ensure carpets maintenance are found in reliable websites such as Carpet and Rug Institute. More so, the companies authorized to sell carpets also have information on ways to take care of the carpets.
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